Table of Deployable Trunked Channels

NPSTC and NRPC Recommended Channels for Deployable Trunked Systems

On February 13, 2015, NPSTC and the NRPC recommended a set of six former reserve channels (12.5 kHz bandwidth) to be allocated nationwide for 700 MHz deployable systems. The NPSTC/NRPC recommended channels are listed below:

|  |  |  |  |
| --- | --- | --- | --- |
| Deployable Trunked Channel | Channel Number | 12.5 kHz Center Frequency | Separation from Lower-Adjacent Deployable Trunked Channel (kHz) |
| A | 37-38 | 769.23125 | N/A |
| B | 61-62 | 769.38125 | 150 |
| C | 117-118 | 769.73125 | 350 |
| D | 141-142 | 769.88125 | 150 |
| E | 883-884 | 774.51875[[1]](#footnote-1) | 4500 |
| F | 939-940 | 774.86875[[2]](#footnote-2) | 350 |

On March 3, the Public Safety and Homeland Security Bureau issued a *Public Notice* seeking comment on the recommended channels.[[3]](#footnote-3) On April 2, 2015, the Association of Public-Safety Communications Officials-International, Inc. filed comments urging approval of the NPSTC/NRPC recommended channels.[[4]](#footnote-4)

Accordingly, we hereby approve the recommended channels as set forth above. RPCs may now incorporate these channels into their plans for deployable trunked systems provided any region with a T-Band market must give priority to these channels, in that market, to any public safety T-band incumbent seeking to relocate from the T-band.[[5]](#footnote-5)

1. NPSTC and NRPC recommend this channel as the primary control channel (CC-P). [↑](#footnote-ref-1)
2. NPSTC and NRPC recommend this channel as the alternate control channel (CC-A). [↑](#footnote-ref-2)
3. *See* Public Safety and Homeland Security Bureau Seeks Comment on Recommended Nationwide Channels for Deployable Trunked Systems in the 700 MHz Narrowband Public Safety Band, *Public Notice,* PS Docket No. 13-87 and WT Docket 02-378, DA 15-278 (PSHSB rel. Mar. 3, 2015). [↑](#footnote-ref-3)
4. *See* Comments of Association of Public-Safety Communications Officials-International, Inc. (Apr. 2, 2015). [↑](#footnote-ref-4)
5. Regional Planning Committees must file plan amendments to reflect the revised 700 MHz narrowband segment no later than October 30, 2015. *See* Proposed Amendments to the Service Rules Governing Public Safety Narrowband Operations in the 769-775/799-805 MHz Bands, *et al*, PS Docket 13-87, PS Docket 06-229, WT Docket 96-86, RM 11433 and RM 11577, *Order*, DA 15-476 (PSHSB rel. Apr. 20, 2015). [↑](#footnote-ref-5)